<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.22.10-Bia?owie?a">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract></abstract>
  <contact>
    <name></name>
    <organization></organization>
    <position></position>
    <voice></voice>
    <fax></fax>
    <email></email>
    <role></role>
  </contact>
  <links/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys>
      <wkt>BOUNDCRS[SOURCECRS[PROJCRS["BD72 / Belgian Lambert 72",BASEGEOGCRS["BD72",DATUM["Reseau National Belge 1972",ELLIPSOID["International 1924",6378388,297,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4313]],CONVERSION["Belgian Lambert 72",METHOD["Lambert Conic Conformal (2SP)",ID["EPSG",9802]],PARAMETER["Latitude of false origin",90,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8821]],PARAMETER["Longitude of false origin",4.36748666666667,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8822]],PARAMETER["Latitude of 1st standard parallel",51.1666672333333,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8823]],PARAMETER["Latitude of 2nd standard parallel",49.8333339,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8824]],PARAMETER["Easting at false origin",150000.013,LENGTHUNIT["metre",1],ID["EPSG",8826]],PARAMETER["Northing at false origin",5400088.438,LENGTHUNIT["metre",1],ID["EPSG",8827]]],CS[Cartesian,2],AXIS["easting (X)",east,ORDER[1],LENGTHUNIT["metre",1]],AXIS["northing (Y)",north,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Engineering survey, topographic mapping."],AREA["Belgium - onshore."],BBOX[49.5,2.5,51.51,6.4]],ID["EPSG",31370]]],TARGETCRS[GEOGCRS["WGS 84",DATUM["World Geodetic System 1984",ELLIPSOID["WGS 84",6378137,298.257223563,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],CS[ellipsoidal,2],AXIS["geodetic latitude (Lat)",north,ORDER[1],ANGLEUNIT["degree",0.0174532925199433]],AXIS["geodetic longitude (Lon)",east,ORDER[2],ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4326]]],ABRIDGEDTRANSFORMATION["BD72 to WGS 84 (1)",VERSION["IGN-Bel 7"],METHOD["Coordinate Frame rotation (geog2D domain)",ID["EPSG",9607]],PARAMETER["X-axis translation",-99.059,ID["EPSG",8605]],PARAMETER["Y-axis translation",53.322,ID["EPSG",8606]],PARAMETER["Z-axis translation",-112.486,ID["EPSG",8607]],PARAMETER["X-axis rotation",-0.419,ID["EPSG",8608]],PARAMETER["Y-axis rotation",0.83,ID["EPSG",8609]],PARAMETER["Z-axis rotation",-1.885,ID["EPSG",8610]],PARAMETER["Scale difference",0.999999,ID["EPSG",8611]],USAGE[SCOPE["(null/copy) Approximation for medium and low accuracy applications assuming equality between plate-fixed static and earth-fixed dynamic CRSs, ignoring static/dynamic CRS differences."],AREA["Belgium - onshore."],BBOX[49.5,2.5,51.51,6.4]],ID["EPSG",1609],REMARK["Scale difference is given by information source as 0.999999. Given in this record in ppm to assist application usage. Very similar parameter values (to slightly less precision) used for BD72 to ETRS89: see code 1652."]]]</wkt>
      <proj4>+proj=lcc +lat_0=90 +lon_0=4.36748666666667 +lat_1=51.1666672333333 +lat_2=49.8333339 +x_0=150000.013 +y_0=5400088.438 +ellps=intl +towgs84=-99.059,53.322,-112.486,0.419,-0.83,1.885,-1 +units=m +no_defs +type=crs</proj4>
      <srsid>0</srsid>
      <srid>0</srid>
      <authid></authid>
      <description>BD72 / Belgian Lambert 72</description>
      <projectionacronym></projectionacronym>
      <ellipsoidacronym>PARAMETER:6378388:6356911.94612794648855925</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial dimensions="2" minz="0" maxx="0" miny="0" maxz="0" maxy="0" crs="" minx="0"/>
    <temporal>
      <period>
        <start></start>
        <end></end>
      </period>
    </temporal>
  </extent>
</qgis>
